N-X10 User Manual

**Factory default**

|  |  |
| --- | --- |
| Programming password | 123456 (default) |
| Open door mode | Card or digital password |
| Lock relay time | Can set (00~99)S |
| Tamper alarm | Open |
| Open card function | Yes |

**Indicator light:**

1. Open the door, the green light is on
2. Enter the programming mode, the green light is always on
3. Standby state, no light
4. The card is not registered, when punch by card, the light turn red.
5. The door open password is wrong, the red light is on.

**Buzzer:**

Valid command: 3 short “beep beep beep”

Invalid command: long “beep”

Full record: 3 long “beep...beep...beep....

Press [\*] to cancel the command: 3 short “beep beep beep” quickly

**Features and settings:**

1. How to change administrator code? (Default: 123456)

Ans: - Press \* # administrator code (Default: 123456) >> Press 0 >> Press 6 digit administrator code >> Again press 6 digit administrator code >> The device will beep 3 times, the setting is successful >> ESC (\*\*).

1. How to add card in device?

Ans: - Press \* # administrator code (Default: 123456) >> Press 5 >> Press 3 digit user ID >> Show card in device >> ESC (\*\*).

Register more cards and repeat the above steps (Example: Press \* # administrator code (Default: 123456) press 5 >> Press 3 digit user ID 001 swipe card >> 002 swipe card >> 003 swipe card... for continuous registration) >> ESC (\*\*).

1. How to delete card in device?

Ans: - Press \* # administrator code (Default: 123456) >> Press 7 >> Show card in device >> ESC (\*\*).

Delete more cards and repeat the above steps (Example: Press \* # Administrator code (Default: 123456) press 6 >> 000, 001, 002... for continuous deletion) >> ESC (\*\*).

1. How to set password? (Only 2 password support in device)

Ans: - Press \* # administrator code (Default: 123456) >> Press 3 >> Press 4 digit password >> Then again press 3 >> Press 4 Digit same password >> The device will beep 3 times, the setting is successful >> ESC (\*\*).

1. How to delete all password?

Ans: - Press \* # administrator code (Default: 123456) >> Press 3 >> 0000 >> The device will beep 3 times, the setting is successful >> ESC (\*\*).

1. How to set lock delay time?

Ans: - Press \* # administrator code (Default: 123456) >> Press 2 >> Set lock delay second (01 to 99) >> ESC (\*\*).

1. Restore factory defaults?

Ans: - Press \* # administrator code (Default: 123456) >> Press 197320 >> ESC (\*\*) The device will beep 3 times, then 3 beeps, wait for about 20 seconds, all setting parameters and data will be restored to the factory default.

(Note: - Please use with caution, all registered data will be deleted and cleared after recovery all user settings).